

d/g/r>

d/g/r>

d/g/r>

d/g/r>h
download to 0x80006020

Ymodem:
CCCCCCC
checksum:0x00036D1D
crc32:0xCF89DEA2, len:0x00000BE4

d/g/r>

d/g/r>

d/g/r>s
98007058

01500000
98007058 = 0x01500000

d/g/r>

d/g/r>

d/g/r>

d/g/r>d
download to 0x01500000

Ymodem:
CCCCCCC
checksum:0x07A29471
crc32:0xA36A16A1, len:0x000B71E0

d/g/r>

d/g/r>

d/g/r>

d/g/r>

d/g/r>g
jump to 0x01500000
64b

======================================

======================================
1295 hw setting. 
.config transform to binary. 
--------------------------
1295 hw setting. 
.config transform to binary. 
--------------------------
Transferring HW setting file
1295 hw setting ...
ready to upload hw setting via ymodem
Sending file via ymodem
send header..
wait return header ack
send 1st done
send all done
send end body
wait return end ack
sendy done
hwstting - scan keyword..
hw setting upload successful
--------------------------
enter flash write.
-- flash write start --
-- burn dvrboot.bin start --
ready to upload bootcode via ymodem
Sending file via ymodem
send header..
wait return header ack
send 1st done
send all done
send end body
wait return end ack
sendy done
scan keyword finish
timeout..
whole procedure is fail
