

d/g/r>

d/g/r>

d/g/r>

d/g/r>h
download to 0x80006020

Ymodem:
CCCCCCC
checksum:0x00036D1D
crc32:0xCF89DEA2, len:0x00000BE4

d/g/r>

d/g/r>

d/g/r>s
98007058

01500000
98007058 = 0x01500000

d/g/r>

d/g/r>

d/g/r>

d/g/r>d
download to 0x01500000

Ymodem:
CCCCCCCC
checksum:0x07ABBEA8
crc32:0x9C4CFD1A, len:0x001427A8

d/g/r>

d/g/r>

d/g/r>

d/g/r>

d/g/r>g
jump to 0x01500000
64b
flash_type: eMMC
begin: 

emmc : PLL_EMMC1 = 0x00000003
emmc : dummy_buffer = 0x00200240, dummy_512B = 0x00200248
switch frequency to 0x00000046
frequency divider is 0x00000080
switch frequency to 0x00000046
frequency divider is 0x00000004
switch to SDR 8 bit
switch bus width to 0x00000008 bits success
-------->disable dcache 
**********for NON_SECURE_BOOT
*******************************************
hwsetting: block 0x00000100, size 0x00000C80
write data to UDA
read hwsetting back: block 0x00000100, size 0x00000C80
read from UDA
*******************************************
write bootcode: block 0x00000107, size 0x0007D920
write data to UDA
read back bootcode: block 0x00000107, size 0x0007D920
read from UDA
*******************************************
*******************************************
write fsbl,fsbl_sig: block 0x000004F4, fsbl size 0x00011900, fsbl_sig_size 0x00000020
write data to UDA
read back data(fsbl/fsbl_sig): block 0x000004F4, fsbl size 0x00011900, fsbl_sig_size 0x00000020
read from UDA
*******************************************
write fsbl_os,fsbl_os_sig: block 0x00000581, fsbl_os size 0x0007BD80, fsbl_os_sig_size 0x00000020
write data to UDA
read back data(fsbl_os/fsbl_os_sig): bloc0ÿ?B”Bk 0x00000581, fsbl_os size 0x0007BD80, fsbl_os_sig_size 0x00000020
read from UDA
*******************************************
write bl31,bl31_sig: block 0x00000960, bl31 size 0x00006280, bl31_sig_size 0x00000020
write data to UDA
read back data(bl31/bl31_sig): block 0x00000960, bl31 size 0x00006280, bl31_sig_size 0x00000020
read from UDA
*******************************************
write extern_param: block 0x0000007C, size 0x800
write data to UDA
read back extern_parm: block 0x0000007C, size 0x00000ÿ?B0800
read from UDA
Finish
Total dump 0x00112C00 at 0x03000000

======================================

======================================
”B1295 hw setting. 
.config transform to binary. 
--------------------------
Setup COM device parameter fail!!
Transferring HW setting file
1295 hw setting ...
ready to upload hw setting via ymodem
Sending file via ymodem
send header..
wait return header ack
send 1st done
send all done
send end body
wait return end ack
sendy done
hwstting - scan keyword..
hw setting upload successful
--------------------------
enter flash write.
-- flash write start --
-- burn dvrboot.bin start --
ready to upload bootcode via ymodem
Sending file via ymodem
send header..
wait return header ack
send 1st done
send all done
send end body
wait return end ack
sendy done
scan keyword finish
finish
whole procedure is done
