===========================================================
burn option:
only upgrade bootloader :1
read flash data :0
read nand flash spare :0
single mode :0
compare mode :0
ues se_storage :0
hack go ddr (only 1195) :0
only upgrade firmware (not include factory area) :0
only program efuse :0
only upgrade secure firmware  (not include prattion and mbr and factory) :0
burn factory :0
NAS enable :0
LK enable :0
===========================================================
ThreadProgramDevice with device index(0) 
flash type : 2.
once max trans range : 0x200000 
trans range : 0x40000
secure : 0
go/Jump : 0
[device table] 
table[0] path = \\?\usb#vid_0bda&pid_1195#0357802115946#{7b56a5d6-cd10-4410-9f59-9a5e71269882}
table[1] path = 
table[2] path = 
table[3] path = 
table[4] path = 
table[5] path = 
table[6] path = 
table[7] path = 
table[8] path = 
table[9] path = 
table[10] path = 
table[11] path = 
thread [0] path = \\?\usb#vid_0bda&pid_1195#0357802115946#{7b56a5d6-cd10-4410-9f59-9a5e71269882} 
prepare usb_hwsetting buffer
prepare usb_hwsetting buffer done
run usb hwsetting icon:[0] 
once max trans total cont : 1 
trans count: 0 
trans total cont : 1 
first start address : 0x1500000
write address : 0x1500000 
Now data remaining length : 0x760 
Now256KCont : 0 
Total256KCont : 1 
bRempFinish : 0 
dataOffsetSeekRange : 0x0 
onceTransSize : 0x760 
iRemainSize : 0x0 
dataToalSize : 0x0 
******************************
******** CBW *** CBWCB *******
CBW.dCBWDataTransferLength : 0x760 
CBW.iIndicator: 3 
CBW.dCbwcb.LogicalBlockAddress : 0x1500000 
******************************

==========================================
===============debug log===================

DONE - Transmission is completed !

===============debug log end==================
==========================================

run usb hwsetting ddr enable icon[0]:
once max trans total cont : 1 
trans count: 0 
trans total cont : 1 
first start address : 0x0
write address : 0x0 
Now data remaining length : 0x0 
Now256KCont : 0 
Total256KCont : 1 

==========================================
===============debug log===================

DONE - Transmission is completed !

===============debug log end==================
==========================================

uboot hwsetting address icon[0] : start block : 256 ¡C
once max trans total cont : 1 
trans count: 0 
trans total cont : 1 
first start address : 0x100
write address : 0x100 
Now data remaining length : 0xc80 
Now256KCont : 0 
Total256KCont : 1 
bRempFinish : 0 
dataOffsetSeekRange : 0x0 
onceTransSize : 0xc80 
iRemainSize : 0x0 
dataToalSize : 0x0 
******************************
******** CBW *** CBWCB *******
CBW.dCBWDataTransferLength : 0xc80 
CBW.iIndicator: 3 
CBW.dCbwcb.LogicalBlockAddress : 0x100 
******************************

==========================================
===============debug log===================

DONE - Transmission is completed !

===============debug log end==================
==========================================

boocode address icon[0] : start block 263 ¡C
once max trans total cont : 1 
trans count: 0 
trans total cont : 1 
first start address : 0x107
write address : 0x107 
Now data remaining length : 0x79ae0 
Now256KCont : 0 
Total256KCont : 2 
bRempFinish : 0 
dataOffsetSeekRange : 0x0 
onceTransSize : 0x40000 
iRemainSize : 0x39ae0 
dataToalSize : 0x39ae0 
******************************
******** CBW *** CBWCB *******
CBW.dCBWDataTransferLength : 0x40000 
CBW.iIndicator: 1 
CBW.dCbwcb.LogicalBlockAddress : 0x107 
******************************
bRempFinish : 0 
dataOffsetSeekRange : 0x40000 
onceTransSize : 0x39ae0 
iRemainSize : 0x0 
dataToalSize : 0x0 
******************************
******** CBW *** CBWCB *******
CBW.dCBWDataTransferLength : 0x39ae0 
CBW.iIndicator: 3 
CBW.dCbwcb.LogicalBlockAddress : 0x107 
******************************

==========================================
===============debug log===================

DONE - Transmission is completed !

===============debug log end==================
==========================================

uboot FSBL address icon[0] : start block : 1237 ¡C
once max trans total cont : 1 
trans count: 0 
trans total cont : 1 
first start address : 0x4d5
write address : 0x4d5 
Now data remaining length : 0x11b20 
Now256KCont : 0 
Total256KCont : 1 
bRempFinish : 0 
dataOffsetSeekRange : 0x0 
onceTransSize : 0x11b20 
iRemainSize : 0x0 
dataToalSize : 0x0 
******************************
******** CBW *** CBWCB *******
CBW.dCBWDataTransferLength : 0x11b20 
CBW.iIndicator: 3 
CBW.dCbwcb.LogicalBlockAddress : 0x4d5 
******************************

==========================================
===============debug log===================

DONE - Transmission is completed !

===============debug log end==================
==========================================

close device icon:[c24]
ThreadProgramDevice with device index(0) end 
